<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<configurations XML_version="1.2" id="configurations_0">
<configuration XML_version="1.2" id="Texas Instruments XDS2xx USB Emulator_0">
        <instance XML_version="1.2" desc="Texas Instruments XDS2xx USB Emulator_0" href="connections/TIXDS2XXUSB_Connection.xml" id="Texas Instruments XDS2xx USB Emulator_0" xml="TIXDS2XXUSB_Connection.xml" xmlpath="connections"/>
        <connection XML_version="1.2" id="Texas Instruments XDS2xx USB Emulator_0">
            <instance XML_version="1.2" href="drivers/tixds560icepick_c.xml" id="drivers" xml="tixds560icepick_c.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds560c64xp.xml" id="drivers" xml="tixds560c64xp.xml" xmlpath="drivers"/>
            <platform XML_version="1.2" id="platform_0">
                <instance XML_version="1.2" desc="TMS320C6455_0" href="devices/c6455.xml" id="TMS320C6455_0" xml="c6455.xml" xmlpath="devices"/>
            <device HW_revision="1" XML_version="1.2" description="TMS320C6455" id="TMS320C6455_0" partnum="TMS320C6455">
                    <router HW_revision="1.0" XML_version="1.2" description="ICEPick_C Router" id="IcePick_C_0" isa="ICEPICK_C">
                        <subpath id="subpath_0">
                            <cpu HW_revision="1.0" XML_version="1.2" description="C64x+ CPU" id="C64XP_0" isa="TMS320C64XP">
                                <property Type="filepathfield" Value="VIB_C6455.gel" id="GEL File"/>
                            </cpu>
                        </subpath>
                    </router>
                </device>
            </platform>
        </connection>
    </configuration>
</configurations>
